# Configure connections for local APs

To define the connection configuration of a local Tuxedo access point that will be used with this WTC Service:

1. If you have not already done so, in the Change Center of the Administration Console, click Lock & Edit (see Use the Change Center).
2. In the Administration Console, expand Interoperability and select WTC Service.
3. On the WTC Servers page, click the name of a WTC Service.
4. Click the Local APs tab.
5. On the WTC Local Access Points page, click the name of a local access point.
6. Click the Connections tab.
7. Modify the connection attributes for your environment.

   See Configuration Options.

8. Click Save.
9. To activate these changes, in the Change Center of the Administration Console, click Activate Changes.
   Not all changes take effect immediately—some require a restart (see Use the Change Center).