> # WTC Server: Configuration: Local APs

> Column Display Related Tasks Related Topics

> Local Tuxedo access points provide configuration information to connect available remote Tuxedo domains to a WTC server. You must have at least one local Tuxedo access point configured to create a WTC server.

> This page summarizes the local Tuxedo access points that have been configured in the current WTC server.

> #### Column Display

> You can show fewer or additional data points on this page by expanding Customize this table and modifying the Column Display list. Each data point displays in its own table column.

> The following table lists all of the data points that you can display in columns on this page.

> Name | Description
> --- | ---
> Name | The unique name used to identify this local Tuxedo access point. This name should be unique for all local and remote Tuxedo access points defined within a WTC Service. This allows you to define unique configurations having the same Access Point ID. MBean Attribute: `WTCLocalTuxDomMBean.AccessPoint`
> Access Point ID | The connection principal name used to identify this local Tuxedo access point when attempting to establish a session connection with remote Tuxedo access points. Note: The AccessPointId must match the corresponding DOMAINID in the *DM_REMOTE_DOMAINS section of your Tuxedo DMCONFIG file. MBean Attribute: `WTCLocalTuxDomMBean.AccessPointId`

> Related Tasks

> - Create local access points
> - Configure connections for local access points
> - Configure security for remote access points
> - Delete local access points

> Related Topics

> - Configuring Oracle WebLogic Tuxedo Connector